(footprint "3_PIN_WIRE"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 2.5 -4 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "ed9aed21-178b-495d-b9e1-929f192a36e4")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "3_PIN_WIRE"
		(at 2.5 -2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "a81b8f00-4fb7-411f-ad2b-943cd5e16966")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "874c5579-03b1-4f97-8e19-7e491326f2e9")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "ac906119-cf33-42dd-9c1a-5d2fb67ab974")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start -1.5 -1.5)
		(end 6.5 1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "3c534895-8b86-4446-afd7-676a7a56e959")
	)
	(fp_text user "${REFERENCE}"
		(at 2.5 3 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "0f18bd78-61ca-451a-9eeb-2263cb5f43f2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 0 0)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0)
		(uuid "ebc9015d-9cc2-4111-aef3-b60d76b89373")
	)
	(pad "2" thru_hole circle
		(at 2.5 0)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0)
		(uuid "173044b5-a2c0-4c4f-bb3f-f9fd466a356c")
	)
	(pad "3" thru_hole circle
		(at 5 0)
		(size 1.75 1.75)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(solder_mask_margin 0)
		(uuid "f499520f-f554-4d82-83ea-fa2da2309ab8")
	)
	(embedded_fonts no)
)
