(footprint "W3213"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 6.5 -10 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "f24b340a-fab5-4a19-89d5-142c860a7fc0")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "W3213"
		(at 6.5 -2.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "04dd6c12-8251-4781-a9f5-1b11f920ff3a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b99134c4-fb24-4473-86ca-b34478a5cd2d")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cd3e3cb1-5955-400e-9a61-613d452727a7")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start 0 -13)
		(end 13 0)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "c78c6db4-7e41-4ecc-83d0-30df1c12f03d")
	)
	(fp_rect
		(start -1 -14)
		(end 14 1)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill no)
		(layer "F.CrtYd")
		(uuid "4539cb55-422e-48bf-a735-c6db2ea37043")
	)
	(fp_text user "${REFERENCE}"
		(at 6.5 -1 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "4e027ed7-f943-4ac4-b64e-958cf24df4e4")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" thru_hole circle
		(at 6.5 -5.8)
		(size 3.6 3.6)
		(drill 2.5)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "e16d3e96-37cd-42db-8a30-66cca71459e4")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(uuid "4534681b-5cec-434f-b51a-fe95ff081411")
		(name "KEEP-OUT")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 0 0.141405) (xy 0 -12.858595) (xy 13 -12.858595) (xy 13 0.141405)
			)
		)
	)
	(embedded_fonts no)
)
