(footprint "PA1010D"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 5.5 -1 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "130f3771-d8e2-4352-9988-833559a1de18")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "PA1010D"
		(at 5 8.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "41b10efd-006f-40fa-bbac-f8ded5a8fb94")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "b21a5dda-2f72-4e25-aec7-67c44f8948ee")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "cc6957af-7fef-407d-948e-2e72ed2fa122")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_rect
		(start 0 0)
		(end 10 10)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill no)
		(layer "F.SilkS")
		(uuid "d57ec54c-ee0b-47c8-a7f8-dc75c8a9b37a")
	)
	(fp_circle
		(center 1.5 1)
		(end 1.5 1.5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill yes)
		(layer "F.SilkS")
		(uuid "edc44674-6cfd-4316-bad3-efc6a576b3ca")
	)
	(fp_circle
		(center 5 5)
		(end 3.5 5)
		(stroke
			(width 0.1)
			(type solid)
		)
		(fill yes)
		(layer "Edge.Cuts")
		(uuid "c34f8951-a402-414f-8c4a-f636b56f109c")
	)
	(fp_text user "${REFERENCE}"
		(at 5 2 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "722d4a1d-7d11-4a0d-8121-59126244e839")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd roundrect
		(at 0 1.15 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "dd90346c-26e8-425a-9a22-9aa95ea9966c")
	)
	(pad "2" smd roundrect
		(at 0 2.75 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "3ed9afe3-fc3d-4c35-8d7a-cc9f3faca37b")
	)
	(pad "3" smd roundrect
		(at 0 5.65 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "baf6929d-7350-437e-b05a-f2d9bce91360")
	)
	(pad "4" smd roundrect
		(at 0 7.25 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "6ec8d1d5-e58f-4b90-9380-ff6ca42c02dd")
	)
	(pad "5" smd roundrect
		(at 0 8.85 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "6f769a41-6d17-4d4a-8d0a-1c53033bec90")
	)
	(pad "6" smd roundrect
		(at 10 8.85 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "8377c02f-ce7c-4edb-af17-6113f49103f3")
	)
	(pad "7" smd roundrect
		(at 10 7.25 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "1b5dcfd8-2351-4f21-91e5-80eb16f68d64")
	)
	(pad "8" smd roundrect
		(at 10 5.65 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "af994bfc-2691-4dd3-a5a6-1b7939aef85f")
	)
	(pad "9" smd roundrect
		(at 10 2.75 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "de6b9b35-3982-456a-8dad-8c11afd9d2a6")
	)
	(pad "10" smd roundrect
		(at 10 1.15 90)
		(size 0.8 1.5)
		(layers "F.Cu" "F.Mask" "F.Paste")
		(roundrect_rratio 0.15)
		(uuid "ed9d7d62-f653-4f37-8d08-2969d1579eea")
	)
	(embedded_fonts no)
)
