EESchema-DOCLIB  Version 2.0
#
$CMP LSM6DSV80XTR
D 6-axis IMU (inertial measurement unit) with high-g accelerometer, embedded AI, and sensor fusion for wearables and sport trackers
K
F https://www.st.com/resource/en/datasheet/lsm6dsv80x.pdf
$ENDCMP
#
#End Doc Library
