(kicad_symbol_lib (version 20211014) (generator SamacSys_ECAD_Model)
  (symbol "LSM6DSV80XTR" (in_bom yes) (on_board yes)
    (property "Reference" "IC" (at 31.75 15.24 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Value" "LSM6DSV80XTR" (at 31.75 12.7 0)
      (effects (font (size 1.27 1.27)) (justify left top))
    )
    (property "Footprint" "LSM6DSV16BXTR" (at 31.75 -87.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Datasheet" "https://www.st.com/resource/en/datasheet/lsm6dsv80x.pdf" (at 31.75 -187.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "ki_description" "6-axis IMU (inertial measurement unit) with high-g accelerometer, embedded AI, and sensor fusion for wearables and sport trackers" (at 31.75 -287.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Height" "0.74" (at 31.75 -387.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Name" "STMicroelectronics" (at 31.75 -487.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Manufacturer_Part_Number" "LSM6DSV80XTR" (at 31.75 -587.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Part Number" "" (at 31.75 -687.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Mouser Price/Stock" "" (at 31.75 -787.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Part Number" "LSM6DSV80XTR" (at 31.75 -887.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (property "Arrow Price/Stock" "https://www.arrow.com/en/products/lsm6dsv80xtr/stmicroelectronics?utm_currency=USD&region=nac" (at 31.75 -987.3 0)
      (effects (font (size 1.27 1.27)) (justify left top) hide)
    )
    (rectangle
      (start 5.08 10.16)
      (end 30.48 -20.32)
      (stroke (width 0.254) (type default))
      (fill (type background))
    )
    (pin passive line (at 0 0 0) (length 5.08)
      (name "SDO/SA0" (effects (font (size 1.27 1.27))))
      (number "1" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -2.54 0) (length 5.08)
      (name "SDX" (effects (font (size 1.27 1.27))))
      (number "2" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -5.08 0) (length 5.08)
      (name "SCX" (effects (font (size 1.27 1.27))))
      (number "3" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 0 -7.62 0) (length 5.08)
      (name "INT1" (effects (font (size 1.27 1.27))))
      (number "4" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 15.24 -25.4 90) (length 5.08)
      (name "VDDIO" (effects (font (size 1.27 1.27))))
      (number "5" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 17.78 -25.4 90) (length 5.08)
      (name "GND_1" (effects (font (size 1.27 1.27))))
      (number "6" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 20.32 -25.4 90) (length 5.08)
      (name "GND_2" (effects (font (size 1.27 1.27))))
      (number "7" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -7.62 180) (length 5.08)
      (name "VDD" (effects (font (size 1.27 1.27))))
      (number "8" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -5.08 180) (length 5.08)
      (name "INT2" (effects (font (size 1.27 1.27))))
      (number "9" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 -2.54 180) (length 5.08)
      (name "NC_1" (effects (font (size 1.27 1.27))))
      (number "10" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 35.56 0 180) (length 5.08)
      (name "NC_2" (effects (font (size 1.27 1.27))))
      (number "11" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 20.32 15.24 270) (length 5.08)
      (name "CS" (effects (font (size 1.27 1.27))))
      (number "12" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 17.78 15.24 270) (length 5.08)
      (name "SCL" (effects (font (size 1.27 1.27))))
      (number "13" (effects (font (size 1.27 1.27))))
    )
    (pin passive line (at 15.24 15.24 270) (length 5.08)
      (name "SDA" (effects (font (size 1.27 1.27))))
      (number "14" (effects (font (size 1.27 1.27))))
    )
  )
)
